LA4485

RETOUR SOMMAIRE DES COMPOSANTS

RETOUR

#
LA4485 Power Amlifier

###
2 x 5 Watt in two-channel mode
15 Watt in BTL mode (Bridge)

Pin | Name | Description
--- | --- | ---
1 | CH1 IN | Channel 1 input
2 | CH2 IN | Channel 2 input
3 | SS GND | Small-signal ground
4 | BTL IN | BTL-mode feedback input
5 | BTL OUT | BTL-mode feedback output
6 | FILTER | Filter capacitor connection
7 | LS Vcc | Large-signal supply
8 | SS Vcc | Small-signal supply
9 | STADBY | Stanby control input
10 | MUTE | Mute control input
11 | CH2 OUT | Channel 2 output
12 | LS GND | Large-signal ground
13 | CH! OUT | Channel 1 out