2SC1674

RETOUR SOMMAIRE DES COMPOSANTS

RETOUR

##
2SC1674
Silicon NPN Transistor
High frequency applications.

### The 2SC1674 is a silicon NPN planar epitaxial transistor in a TO-92 type package. This device is suitable for use as FM RF amplifier, Mixer and IF amlifier applications.

| ECB

Absolute Maximum Ratings: (TA = +25°C unless otherwise specified)

Collector-Base Voltage, VCBO | 30V
Collector-Emitter Voltage, VCEO | 20V
Emitter-Base Voltage, VEBO | 4V
Collector Current, IC | 20mA
Total Device Dissipation (TA = +25°C), PD | 250mW
Operating Junction Temperature, TJ | +125°C
Storage Temperature Range, Tstg | -55° to +125°C

Electrical Characteristics:
(TA = +25°C unless otherwise specified)

Parameter | Symbol | Test Conditions | Min | Typ | Max | Unit
Forward Current Transfer Ratio | hFE | VCE = 6V, IC = 1mA | 40 | 90 | 180 |
Current Gain-Bandwidth Product | fT | IC = 5mA, VCE = 6V, IE | 400 | 600 | - | MHz
Power Gain | PG | VCE = 6V, IC = 1mA, f = 100MHz | 18 | 22 | - | dB
Noise Figure | NF | IC = 1mA, VCB = 6V, f = 100MHz | - | 3 | 5 | dB