TK10930

RETOUR SOMMAIRE DES COMPOSANTS

RETOUR

#
TK10930V Narrowband FM/AM IF Amplifire and Demodulator

Narrow band FM/AM IF system lC (for use in amateur, air band, marine band receivers)up to 60MHz.
Features
AM/FM IF Amp. available : Independent operation.
Wide operating voltage range : 2.5V 8.0V.
Wide signal meter output.
AGC amp. for AM IF available.
Ceramic discriminator is available.
AM ON/OFF Function

Pin | Name | Description
--- | --- | ---
1 |  | Oscillator
2 |  | Oscillator
3 |  | Mixer Out
4 | Vcc | Positive Power Supply
5 |  | AM IF Output
6 |  | Decoupling
7 |  | FM IF Output
8 |  | Decoupling
9 |  | Decoupling
10 |  | Limiter Output
11 |  | Quad In
12 |  | FM Discriminator Output
13 |  | AM Detector Output
14 |  | AM Switch
15 | GND | IF Ground
16 |  | RSSI Out
17 |  | AM Low Out
18 |  | AM AGC (AutomaticGainControl)
19 |  | Noise Amplifier Input
20 |  | Noise Amplifier Output
21 |  | CCMP In
22 |  | CCMP Out
23 | GND | Mixer Ground
24 |  | RF/IF Input