2SD1667

RETOUR SOMMAIRE DES COMPOSANTS

RETOUR

##
2SD1667 NPN Transistor
50 Volt 5 Ampere 25 Watt

### The 2SB1143 and 2SD1683 is a silicon PNP/NPN epitaxial planer type transistor in TO-220ML package, designed for Relay drivers, high-speed inverters, and other general high-current switching applications.

| B C E

Absolute Maximum Ratings: (TC = +25°C unless otherwise specified)

Collector-Emitter Voltage (RBE = Infinity), VCEO | 50V
Collector-Base Voltage, VCBO | 60V
Emitter-Base Voltage, VEBO | 6V
Collector Current, IC | 5A
Collector Power Dissipation (TA = +25°C), PD | 2W
Collector Power Dissipation (TC = +50°C), PD | 25W
Operating Junction Temperature, TJ | +150°C
Storage Temperature Range, Tstg | -55° to +150°C