uPC1028H

RETOUR SOMMAIRE DES COMPOSANTS

RETOUR

#
uPC1028H FM IF Amplifier and Discriminator

###
Similar to AN5215 AN5730 AN5732 TA7130P LA1150 KA2245 KIA7130 SK3487 and BA403

3 stage differential IF amplifier.
Differential peak detector.
Easy adjustment.
Large output voltage.
Good limiter characteristic.
Wide operating voltage.
Low distortion.
Fewer peripheral parts.
Excellent AM rejection ratio.

Pin | Name | Description
--- | --- | ---
1 |  | Balanced Input
2 |  | Balanced Input
3 | Vcc | Positive Power Supply
4 | GND | Ground
5 |  | + Detector input (Discriminator Coil)
6 |  | - Detector input (Discriminator Coil)
7 |  | Audio Output